Program Release Information
DL-No. DLKM_BT2512071EN

Product name: bizhub C287i/28C-7i, C286i/28C-6i Series

Subject: <Periodic> [bizhub C287i/28C-7i, C286i/28C-6i Series] [FW ver. GC4-SA] Function Version 2.3 Periodic ROM

2025/12/16


1. Release version and download file name

The newly released program version and download file name is as follows.

<C257i, MFP firmware>
*This firmware can use for Multi-Language. (Multi-Language firmware is the same as this firmware.)

**To build FW-Package MSG1-8C copy the FW to USB-Stick, then run the batch file mkMSGx.bat from root**
	Model
	Program Name
	Current Ver.
	New Ver.
	Program File Name
	Languages*

	bizhub C257i
25C-7i
	MFP firmware
	GC2-SA
	GC4-SA
	ACM10Y0-F232-GC4-SA-990-CHECKSUM-bbb5.ZIP
	mkMSGx.bat

(en, de, fr, it, nl)


* mkMSG1.bat (english, german, french, italian, dutch)

* mkMSG2.bat (english, danish, swedish, norwegian, finnish)

* mkMSG3.bat (english, greek, turkish, russian, ukrainian, bulgarian, estonian, lithuanian, latvian)

* mkMSG4.bat (english, czech, polish, slovak, romanian)

* mkMSG5.bat (english, spanish, portuguese, catalan, basque)

* mkMSG6.bat (english, german, croatian, slovenian)

* mkMSG7.bat (english, spanish, portuguese, hungarian)

* mkMSG8A.bat (english, french, arabic)

* mkMSG8B.bat (english, french, hebrew)

* mkMSG8C.bat (english, welsh)
* New version includes contents of base version.

　Please refer to "RFKM_BT2414564EN" for the countermeasures included in this firmware.
 [Download File Name]
ACM10Y0-F232-GC4-SA-990-CHECKSUM-bbb5.DOC (This file)

ACM10Y0-F232-GC4-SA-990-CHECKSUM-bbb5.ZIP

2. What changed
2.1 Release of <Periodic> [bizhub C287i/28C-7i, C286i/28C-6i Series] [FW ver. GC4-SA] Function Version 2.3 Periodic ROM

The individual files are as follows.

	Program Name
	File Name
	Note

	MFP Card Version
	ACM10Y0-F232-GC4-SA
	　

	Linux-based MFP Controller
	Linux-4.4.8
	　

	MFP Controller Kernel Program
	ACM10Y0-1C00-G00-J0
	　

	MFP Controller Subset
	ACM10Y0-1F00-GC1-SA
	　

	MFP Controller
	ACM10Y0-0100-GC4-SA
	　

	MFP Controller System
	ACM10Y0-1000-GC4-SA
	　

	MFP Controller Print Controller
	ACM10Y0-3000-GC0-S5
	　

	MFP Controller Print Controller Font
	ACM10Y0-3F00-GC0-S0
	　

	MFP Controller Print Controller Demo Page
	ACM10Y0-3E00-G00-00
	　

	Image Reader Controller
	ACM10Y0-8600-G00-G3
	　

	MFP Controller MIO
	ACM10Y0-5000-G00-E3
	　

	MFP Controller PIC
	ACM10Y0-8200-G00-N3
	　

	FAX board controller
	A8790Y0-4000-G00-36
	　

	Operation panel message data
	ACM10Y0-8100-G00-TC
	　

	MFP Controller OSL
	AA7N0Y0-G000-GC0-55
	　

	MFP Controller CHR
	ACVX0Y0-G100-GC1-MC
	　

	MFP Controller NDJ
	AA7N0Y0-G200-G25-47
	　

	MFP Controller UPL
	AA7N0Y0-G300-G20-20
	　

	ADF
	AAJ40Y0-0024-G10-02
	　

	Machine Controller
	ACM10Y0-0200-G00-29
	　

	Machine Controller Printer
	ACM10Y0-0220-G00-29
	　

	Machine Controller Media
	ACM10Y0-0230-G00-00
	　

	Machine Controller Scanner
	ACM10Y0-0300-G00-03
	　

	Finisher (FS-533)
	A2YU0Y0-0071-G10-05
	　

	Finisher (FS-539)
	AAR40Y0-0071-G00-20
	　

	Finisher (FS-542)
	ADDC0Y0-0071-G00-04
	　

	Separator (JS-506)
	A2YV0Y0-0070-G00-01
	　

	Separator (JS-506 ARM)
	A2YV0Y0-0070-G10-01
	　

	SD (FS-539SD/540SD)
	A3ER0Y0-0071-G20-06
	　

	OCR Library
	AA2J0Y0-B000-G00-01
	　

	Integrated Printer Driver Version
	6-2.3c-0-GC4-SA
	　


2.2. Addition of function/ Change of specifications

  None

2.3. Fixed issues

1. Email sending may fail due to expiration of OAuth2.0 token.

    [INC000000076822/INC000000046770, INC000000076956/INC000000046934, INC000000076869/INC0543652, INC000000076959/INC0542833, INC000000076873/INC0544034, INC000000076958/PBM-00015165, INC000000077524/INC000000048164, INC000000077414/INC000000047904, INC000000077176/INC000000047274, INC000000077156/INC000000047141]

    *Please refer to PSKM_BT2511727EN for more details,

2. After the G00-S7 firmware was applied, trouble code C-E301 has been occurring on multiple MFPs.[INC000000076615/INC0531872]

3. Web Connection is intermittently inaccessible on FW G00-S7.

    [INC000000077045/INC0549481,INC000000077067/INC0551996,INC000000077201/INC0551893,INC000000077231/INC0554850,INC000000077233/INC0555060,INC000000077314/INC0556342]

4. If Authentication Attack Detection is enabled on the machine, printing multiple files at once via SafeQ Print may result in job errors caused by authentication errors.[INC000000077346/INC0559256]

    *Please refer to PSKM_BT2512042EN for more details,

5. Performing Scan/Fax job changes "Fax Header Settings" to OFF when FW G00-S7 is installed.[INC000000076582 /PBM-00015059]

    *Please refer to PSKM_BT2511638EN for more details,

6.  A site other than the homepage is displayed when opening a web browser after logging in on a PaperCut-managed machine with GC2-SA version installed.[INC000000077701,INC000000077702 /INC000000048611,INC000000048557]

    *Please refer to PSKM_BT2512044EN for more details,

2.4. Customization

  None

3. Cautions and Restrictions
Instead of the correct software keyboard the classic keyboard is shown. [INC0149189]

For croatian/estonian/lithuanian/latvian/welsh keyboard the english keyboard is shown.

For croatian/estonian/lithuanian/latvian/bulgarian/ukrainian WebBrowser the english WebBrowser is shown.

The latest version of the driver/applications as of October 31, 2025 are attached.
-Machines produced with this FW are required to change the administrator's password when MFP is started to be used. Please change the administrator's password before operating the machine.
-Please refer to “Version down method from G00-S7.pdf” when downgrading from this FW to the old FW.
-Please refer to "PSKM_BT2511270EN" when replacing the CPU board or the storage board on the machine with this FW applied,
PDF/A scan function is standardized in the firmware G00-E9 and later versions.

Therefore, PDF/A function that was provided by LK-102 will be enabled once the firmware is installed. If PDF/A Font Data is not installed, the error message will be displayed.

Please be sure confirm PDF/A Font Data is installed in the machine when installing this firmware. Refer KNOVA-PS "PSKM_BT2022690EN" for details.

*When using firmware G00-S7 or later, make sure to use Universal Printer Driver version 3.9.818.0 or newer.
Printing from a PC may fail if an older driver is used.
*When updating from firmware versions prior to Gxx-RF to G00-S7 or later, the system will perform an internal data reconfiguration during the first startup after the firmware update.
Do not turn off the power for 2 minutes after startup.
4. System Requirements
None

5. How to install
Refer to “IT6_Gxx-S7_LDD_installation_procedure.pdf” when updating the FW on a machine with a LDD installed.
Please refer to Service Manual.

<Function Version>

  About Software Switch Settings

    Switch No.: 25

      HEX Assignment: 10 -> Function Version 2.0

      HEX Assignment: 20 -> Function Version 2.1

      HEX Assignment: 30 -> Function Version 2.2

      HEX Assignment: 40 -> Function Version 2.3

6. OpenAPI supported function level
The following is OpenAPI supported function level on this firmware.

OpenAPI:

	OpenAPI Function Level
	5.7.1


Detail:

	Auth
	3.5/3.6/3.7/4.0/4.1/4.2/4.5/4.6/4.7/4.8/4.9/4.10/4.11/4.12/4.13/5.0/5.1/5.5/5.7

	Scan to Application
	3.5/3.6/3.7/4.0/4.5/4.6/4.8/4.9/4.10/4.12

	PullPrint
	3.5/3.6/4.0/4.5/4.6/4.7/4.8/4.9/4.10/4.12/4.13

	Other A
	3.5/4.0

	Job Management
	3.5/3.6/4.0/4.10

	Setup
	3.5/3.6/3.7/3.8/4.0/4.1/4.2/4.5/4.6/4.7/4.8/4.9/4.10/4.11/4.12/
4.13/5.0/5.1/5.2/5.3/5.4/5.5/5.6/5.7

	Link
	4.5/4.6/4.7/4.8/4.9/4.10/4.11/4.12/4.13/5.0/5.1/5.5

	Web Browse
	Auth
	3.5/3.6/3.7/4.0/4.1/4.2/4.5/4.7/4.8/4.9/4.10/4.11/4.13/5.0/5.1/5.5/5.7

	
	Scan to Application
	3.5/3.6/3.7/4.0/4.1/4.5/4.6/4.7/4.8/4.9/4.10/4.12

	
	PullPrint
	3.5/3.6/4.0/4.1/4.5/4.8/4.9/4.10/4.12/4.13

	
	ScrSvr
	3.5/4.0

	
	Launcher
	3.5/4.0/4.8

	
	General
	4.0/4.1/4.5/4.6/4.8/4.9/4.10/4.12/4.13/5.5


7. IWS supported function level
	IWS function Level
	4.2.0


8. Notes
None

* Company names and product names in this document are the registered trademarks for respective companies.
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